**SECTION 09 78 33 – INTERIOR WOOD PANELING**

1. **GENERAL**
	1. SUBMITTALS
		1. Action Submittals:
			1. Product Data: Manufacturer’s descriptive data and product attributes for wood materials.
			2. Samples: Verification samples.
	2. QUALITY ASSURANCE
		1. Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.
		2. Mockup: Minimum [\_\_ x \_\_] feet. Approved mockup [may] [may not] remain as part of the Work.
2. **PRODUCTS**
	1. MANUFACTURERS
		1. Contract Documents are based on products by ThermoryUSA, [www.thermoryusa.com](http://www.thermoryusa.com).
		2. Substitutions: [Refer to Division 01.] [Not permitted.]
	2. MATERIALS
		1. Interior Wood Paneling:
			1. Species: Thermo Aspen.
			2. Profile: STS4.
			3. Size: Nominally [1 x 4] [1 x 5] inches.
		2. Interior Wood Paneling:
			1. Species: Thermo Aspen.
			2. Profile: STEP.
			3. Size: Nominally 5/4 x 3 inches.
		3. Interior Wood Paneling:
			1. Species: Thermo Aspen.
			2. Profile: Kyte.
			3. Size: Nominally 1 x 4 inches.
		4. Interior Wood Paneling:
			1. Species: Thermo Aspen.
			2. Profile: Vire.
			3. Size: Nominally 1 x 4 inches.
		5. Interior Wood Paneling:
			1. Species: Thermo Aspen.
			2. Profile: SHP.
			3. Size: Nominally [1 x 4] [5/4 x 4] inches.
		6. Interior Wood Paneling:
			1. Species: Alder.
			2. Profile: STS4.
			3. Size: Nominally [1 x 4] [1 x 5] inches.
		7. Interior Wood Paneling:
			1. Species: Alder.
			2. Profile: STEP.
			3. Size: Nominally 5/4 x 3 inches.
		8. Interior Wood Paneling:
			1. Species: Alder.
			2. Profile: SHP.
			3. Size: Nominally [1 x 4] [5/4 x 4] inches.
		9. Interior Wood Paneling:
			1. Species: Thermo Magnolia.
			2. Profile: STS10.
			3. Size: Nominally 1 x 7 inches.
		10. Interior Wood Paneling:
			1. Species: Thermo Magnolia.
			2. Profile: SHP.
			3. Size: Nominally 1 5/4 x 4 inches.
		11. Interior Wood Paneling:
			1. Species: Thermo Spruce.
			2. Profile: STS4.
			3. Size: Nominally 1 x 4 inches.
		12. Interior Wood Paneling:
			1. Species: Thermo Spruce.
			2. Profile: SHP.
			3. Size: Nominally 5/4 x 4 inches.
	3. ACCESSORIES
		1. Fasteners: [Plain steel] [Hot-dip galvanized steel] [Stainless steel] [screws.] [nails.]
3. **EXECUTION**
	1. INSTALLATION
		1. Install in accordance with manufacturer's instructions.
		2. Fasten at maximum [12] [16] [\_\_] inches on center.

END OF SECTION